mov ax,0100h

mov es,ax

mov di,0300h

mov ax, 0BCDEh

mov cx, 128

rep stosw

ret

MOV AX,0100h

MOV ES,AX

MOV DS,AX

MOV DI,0300h

MOV SI,0300h

MOV AX, 0BCDEh

MOV CX, 128

CLD

REP STOSW

MOV SI,0300h

MOV DI,0300h

MOV CX, 128

MOV DX, 1234h

dongu:

LODSW

SUB AX,DX

STOSW

LOOP dongu

RET

MOV AX,100h;

MOV ES,AX

MOV DI,0300h

MOV AX, 0BCDEh

MOV CX, 128

CLD

REP STOSW

MOV AX,100h

MOV DS,AX

MOV ES,AX

MOV SI,0300h

MOV DI,3500h;

MOV CX,128

REP MOVSW

RET