MOV AX, 100h

MOV DS, AX

MOV [1000h], 34h

MOV [2000h], 34h

Ret

-----------------------------------------

;ilk degerler

MOV CL, 0CCh

MOV DL, 0DDh

;program

MOV AL, CL

MOV CL, DL

MOV DL, AL

Ret

-----------------------------------------

MOV AX, 100h

MOV DS, AX

MOV [0500h], 9Bh

MOV [0501h], 52h

MOV AX, 00h

MOV AL, [0500h]

MOV AH, [0501h]

ADD AL, AH

MOV [0502h], AL

Ret